LP(4)

NAME
lp - line printer

DESCRIPTION
The lp device refers to the line printer attached to the parallel port. Any byte written to this device is printed. Only one process may have the device open.

The write (2) call may return with a smaller count then the number of bytes requested to write. The next write call is then likely to fail with the error code EAGAIN if the printer is out of paper, or EIO if the printer is turned off.

FILES

/dev/lp
    Parallel port device.

SEE ALSO
lp(1).

BUGS
Only one parallel port is supported.

AUTHOR
Kees J. Bot (kjb@cs.vu.nl)